Employ compute function to calculate input given set point and current velocity

Prints calculated computation

Initialize PID controller using the PID class with certain gain values